# Energized Work Permit

|  |  |  |
| --- | --- | --- |
| Part I: To be completed by the requestor or supervisor of the job | | |
| Requestor’s Name and title: | Request Date: | |
| Description of Equipment: | Job # and Location: | |
| Description of Work to Be Done: | | |
| Justification of why the equipment cannot be de-energized or the work delayed until the next scheduled outage: | | |
| **Part II: To be completed by the qualified person(s) completing the work. Attach responses on separate page(s) if necessary.**  **Check when Complete** | | |
| Hazards present while system remains energized: | | 🞎 |
| Detailed description of procedure to be used in performing the above work: | | 🞎 |
| Description of safe work practices to be employed: | | 🞎 |
| Voltage exposure (shock hazard analysis): | | 🞎 |
| Determination of shock protection boundaries: | | 🞎 |
| Results of flash hazard analysis: | | 🞎 |
| Determination of flash protection boundaries: | | 🞎 |
| PPE required to safely perform the task: | | 🞎 |
| Method used to restrict access to the work area: | | 🞎 |
| Do you agree the above work can be done safely? YES \_\_\_ (proceed to Part III) NO \_\_\_\_ (return to requestor)  **Qualified Person:**   **Name Title Signature Date**  \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_  \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_  \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_ | | |
| **Part III: To be completed by LLE Safety Officers** | | |
| **Approvals:**   **Name Title Signature Date**  \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_  \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_  \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_ | | |
| **Note:** ***Route Permit to LLE Safety Officers***. A minimum of two safety officers must approve energized work. When job is finished, forward to Chief Safety Officer for review and retention. | | |